##############
#
# 64-bit app
#
##############

[dpdk@localhost dpdk-stable-21.11.2-backup]$ sudo ./build-64/app/dpdk-testpmd --lcores=0@2,1@3 -n 6 --socket-mem=1024 -a 07:00.0 -a 08:00.0 --log-level=8 -- -i --rxq=1 --txq=1 --rxd=1024 --txd=1024 --forward-mode=mac
EAL: Detected CPU lcores: 4
EAL: Detected NUMA nodes: 1
EAL: Detected static linkage of DPDK
EAL: Multi-process socket /var/run/dpdk/rte/mp_socket
EAL: Selected IOVA mode 'PA'
EAL: No available 1048576 kB hugepages reported
EAL: Probe PCI driver: net_virtio (1af4:1041) device: 0000:07:00.0 (socket 0)
virtio_init_queue(): vq->vq_ring_mem: 0x154fab000
virtio_init_queue(): vq->vq_ring_virt_mem: 0x1401ab000
virtio_init_queue(): vq->vq_ring_mem: 0x154fa6000
virtio_init_queue(): vq->vq_ring_virt_mem: 0x1401a6000
virtio_init_queue(): vq->vq_ring_mem: 0x154f9a000
virtio_init_queue(): vq->vq_ring_virt_mem: 0x14019a000
EAL: Probe PCI driver: net_virtio (1af4:1041) device: 0000:08:00.0 (socket 0)
virtio_init_queue(): vq->vq_ring_mem: 0x154f91000
virtio_init_queue(): vq->vq_ring_virt_mem: 0x140191000
virtio_init_queue(): vq->vq_ring_mem: 0x154f8c000
virtio_init_queue(): vq->vq_ring_virt_mem: 0x14018c000
virtio_init_queue(): vq->vq_ring_mem: 0x154f80000
virtio_init_queue(): vq->vq_ring_virt_mem: 0x140180000
TELEMETRY: No legacy callbacks, legacy socket not created
Interactive-mode selected
Set mac packet forwarding mode
testpmd: create a new mbuf pool <mb_pool_0>: n=155456, size=2176, socket=0
testpmd: preferred mempool ops selected: ring_mp_mc
Configuring Port 0 (socket 0)
Port 0: 52:54:00:AD:5C:6B
Configuring Port 1 (socket 0)
Port 1: 52:54:00:AC:4D:41
Checking link statuses...
Done
testpmd> set promisc 0 off
testpmd> set promisc 1 off
testpmd> set allmulti 0 on
testpmd> set allmulti 1 on
testpmd> set nbcore 1
Number of forwarding cores set to 1
testpmd> set eth-peer 0 12:34:56:78:9a:bc
testpmd> set eth-peer 1 12:34:56:78:9a:bc
testpmd>
testpmd> show port info all

********************* Infos for port 0  *********************
MAC address: 52:54:00:AD:5C:6B
Device name: 07:00.0
Driver name: net_virtio
Firmware-version: not available
Devargs:
Connect to socket: 0
memory allocation on the socket: 0
Link status: up
Link speed: Unknown
Link duplex: full-duplex
Autoneg status: On
MTU: 1500
Promiscuous mode: disabled
Allmulticast mode: enabled
Maximum number of MAC addresses: 64
Maximum number of MAC addresses of hash filtering: 0
VLAN offload:
  strip off, filter off, extend off, qinq strip off
No RSS offload flow type is supported.
Minimum size of RX buffer: 64
Maximum configurable length of RX packet: 9728
Maximum configurable size of LRO aggregated packet: 0
Current number of RX queues: 1
Max possible RX queues: 1
Max possible number of RXDs per queue: 32768
Min possible number of RXDs per queue: 32
RXDs number alignment: 1
Current number of TX queues: 1
Max possible TX queues: 1
Max possible number of TXDs per queue: 32768
Min possible number of TXDs per queue: 32
TXDs number alignment: 1
Max segment number per packet: 65535
Max segment number per MTU/TSO: 65535
Device capabilities: 0x0( )

********************* Infos for port 1  *********************
MAC address: 52:54:00:AC:4D:41
Device name: 08:00.0
Driver name: net_virtio
Firmware-version: not available
Devargs:
Connect to socket: 0
memory allocation on the socket: 0
Link status: up
Link speed: Unknown
Link duplex: full-duplex
Autoneg status: On
MTU: 1500
Promiscuous mode: disabled
Allmulticast mode: enabled
Maximum number of MAC addresses: 64
Maximum number of MAC addresses of hash filtering: 0
VLAN offload:
  strip off, filter off, extend off, qinq strip off
No RSS offload flow type is supported.
Minimum size of RX buffer: 64
Maximum configurable length of RX packet: 9728
Maximum configurable size of LRO aggregated packet: 0
Current number of RX queues: 1
Max possible RX queues: 1
Max possible number of RXDs per queue: 32768
Min possible number of RXDs per queue: 32
RXDs number alignment: 1
Current number of TX queues: 1
Max possible TX queues: 1
Max possible number of TXDs per queue: 32768
Min possible number of TXDs per queue: 32
TXDs number alignment: 1
Max segment number per packet: 65535
Max segment number per MTU/TSO: 65535
Device capabilities: 0x0( )
testpmd>
testpmd> show port config all
Bad arguments
testpmd> show config fwd
mac packet forwarding - ports=2 - cores=1 - streams=2 - NUMA support enabled, MP allocation mode: native
Logical Core 1 (socket 0) forwards packets on 2 streams:
  RX P=0/Q=0 (socket 0) -> TX P=1/Q=0 (socket 0) peer=12:34:56:78:9A:BC
  RX P=1/Q=0 (socket 0) -> TX P=0/Q=0 (socket 0) peer=12:34:56:78:9A:BC

testpmd> start
mac packet forwarding - ports=2 - cores=1 - streams=2 - NUMA support enabled, MP allocation mode: native
Logical Core 1 (socket 0) forwards packets on 2 streams:
  RX P=0/Q=0 (socket 0) -> TX P=1/Q=0 (socket 0) peer=12:34:56:78:9A:BC
  RX P=1/Q=0 (socket 0) -> TX P=0/Q=0 (socket 0) peer=12:34:56:78:9A:BC

  mac packet forwarding packets/burst=32
  nb forwarding cores=1 - nb forwarding ports=2
  port 0: RX queue number: 1 Tx queue number: 1
    Rx offloads=0x0 Tx offloads=0x0
    RX queue: 0
      RX desc=1024 - RX free threshold=0
      RX threshold registers: pthresh=0 hthresh=0  wthresh=0
      RX Offloads=0x0
    TX queue: 0
      TX desc=1024 - TX free threshold=0
      TX threshold registers: pthresh=0 hthresh=0  wthresh=0
      TX offloads=0x0 - TX RS bit threshold=0
  port 1: RX queue number: 1 Tx queue number: 1
    Rx offloads=0x0 Tx offloads=0x0
    RX queue: 0
      RX desc=1024 - RX free threshold=0
      RX threshold registers: pthresh=0 hthresh=0  wthresh=0
      RX Offloads=0x0
    TX queue: 0
      TX desc=1024 - TX free threshold=0
      TX threshold registers: pthresh=0 hthresh=0  wthresh=0
      TX offloads=0x0 - TX RS bit threshold=0
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 1001       RX-missed: 0          RX-bytes:  84235
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 384        TX-errors: 0          TX-bytes:  16128

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 1001       RX-missed: 0          RX-bytes:  42140
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 486        TX-errors: 0          TX-bytes:  40897

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> clear port stats all

  NIC statistics for port 0 cleared

  NIC statistics for port 1 cleared
testpmd>
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 5          TX-errors: 0          TX-bytes:  210

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:           88
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 5          RX-missed: 0          RX-bytes:  210
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:           88
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 8          TX-errors: 0          TX-bytes:  336

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            1          Tx-bps:          376
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 8          RX-missed: 0          RX-bytes:  336
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            1          Rx-bps:          376
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 5          RX-missed: 0          RX-bytes:  210
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 12         TX-errors: 0          TX-bytes:  504

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          128
  Tx-pps:            0          Tx-bps:           96
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 12         RX-missed: 0          RX-bytes:  504
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 5          TX-errors: 0          TX-bytes:  210

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:           96
  Tx-pps:            0          Tx-bps:          128
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 7          RX-missed: 0          RX-bytes:  294
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 12         TX-errors: 0          TX-bytes:  504

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          328
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 12         RX-missed: 0          RX-bytes:  504
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 7          TX-errors: 0          TX-bytes:  294

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:          328
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 9          RX-missed: 0          RX-bytes:  378
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 12         TX-errors: 0          TX-bytes:  504

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          280
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 12         RX-missed: 0          RX-bytes:  504
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 9          TX-errors: 0          TX-bytes:  378

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:          280
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 11         RX-missed: 0          RX-bytes:  462
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 12         TX-errors: 0          TX-bytes:  504

  Throughput (since last show)
  Rx-pps:            1          Rx-bps:          376
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 12         RX-missed: 0          RX-bytes:  504
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 11         TX-errors: 0          TX-bytes:  462

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            1          Tx-bps:          376
  ############################################################################
testpmd> exit
Command not found
testpmd> quit
Telling cores to stop...
Waiting for lcores to finish...

  ---------------------- Forward statistics for port 0  ----------------------
  RX-packets: 15             RX-dropped: 0             RX-total: 15
  TX-packets: 12             TX-dropped: 105           TX-total: 117
  ----------------------------------------------------------------------------

  ---------------------- Forward statistics for port 1  ----------------------
  RX-packets: 12             RX-dropped: 0             RX-total: 12
  TX-packets: 15             TX-dropped: 3             TX-total: 18
  ----------------------------------------------------------------------------

  +++++++++++++++ Accumulated forward statistics for all ports+++++++++++++++
  RX-packets: 27             RX-dropped: 0             RX-total: 27
  TX-packets: 27             TX-dropped: 108           TX-total: 135
  ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

Done.

Stopping port 0...
Stopping ports...
Done

Stopping port 1...
Stopping ports...
Done

Shutting down port 0...
Closing ports...
Port 0 is closed
Done

Shutting down port 1...
Closing ports...
Port 1 is closed
Done

Bye...
[dpdk@localhost dpdk-stable-21.11.2-backup]$

##############
#
# 32-bit app
#
##############

[dpdk@localhost dpdk-stable-21.11.2-backup]$ sudo ./build-32/app/dpdk-testpmd --lcores=0@2,1@3 -n 6 --socket-mem=1024 -a 07:00.0 -a 08:00.0 --log-level=8 -- -i --rxq=1 --txq=1 --rxd=1024 --txd=1024 --forward-mode=mac
[sudo] password for dpdk:
EAL: Detected CPU lcores: 4
EAL: Detected NUMA nodes: 1
EAL: Detected static linkage of DPDK
EAL: Multi-process socket /var/run/dpdk/rte/mp_socket
EAL: Selected IOVA mode 'PA'
EAL: No available 1048576 kB hugepages reported
EAL: Probe PCI driver: net_virtio (1af4:1041) device: 0000:07:00.0 (socket 0)
virtio_init_queue(): vq->vq_ring_mem: 0x154fb1000
virtio_init_queue(): vq->vq_ring_virt_mem: 0xb6bb1000
virtio_init_queue(): vq->vq_ring_mem: 0x154fad000
virtio_init_queue(): vq->vq_ring_virt_mem: 0xb6bad000
virtio_init_queue(): vq->vq_ring_mem: 0x154fa1000
virtio_init_queue(): vq->vq_ring_virt_mem: 0xb6ba1000
EAL: Probe PCI driver: net_virtio (1af4:1041) device: 0000:08:00.0 (socket 0)
virtio_init_queue(): vq->vq_ring_mem: 0x154f99000
virtio_init_queue(): vq->vq_ring_virt_mem: 0xb6b99000
virtio_init_queue(): vq->vq_ring_mem: 0x154f95000
virtio_init_queue(): vq->vq_ring_virt_mem: 0xb6b95000
virtio_init_queue(): vq->vq_ring_mem: 0x154f89000
virtio_init_queue(): vq->vq_ring_virt_mem: 0xb6b89000
TELEMETRY: No legacy callbacks, legacy socket not created
Interactive-mode selected
Set mac packet forwarding mode
testpmd: create a new mbuf pool <mb_pool_0>: n=155456, size=2176, socket=0
testpmd: preferred mempool ops selected: ring_mp_mc
Configuring Port 0 (socket 0)
Port 0: 52:54:00:AD:5C:6B
Configuring Port 1 (socket 0)
Port 1: 52:54:00:AC:4D:41
Checking link statuses...
Done
testpmd> set promisc 0 off
testpmd> set promisc 1 off
testpmd> set allmulti 0 on
testpmd> set allmulti 1 on
testpmd> set nbcore 1
Number of forwarding cores set to 1
testpmd> set eth-peer 0 12:34:56:78:9a:bc
testpmd> set eth-peer 1 12:34:56:78:9a:bc
testpmd>
testpmd> show port info all

********************* Infos for port 0  *********************
MAC address: 52:54:00:AD:5C:6B
Device name: 07:00.0
Driver name: net_virtio
Firmware-version: not available
Devargs:
Connect to socket: 0
memory allocation on the socket: 0
Link status: up
Link speed: Unknown
Link duplex: full-duplex
Autoneg status: On
MTU: 1500
Promiscuous mode: disabled
Allmulticast mode: enabled
Maximum number of MAC addresses: 64
Maximum number of MAC addresses of hash filtering: 0
VLAN offload:
  strip off, filter off, extend off, qinq strip off
No RSS offload flow type is supported.
Minimum size of RX buffer: 64
Maximum configurable length of RX packet: 9728
Maximum configurable size of LRO aggregated packet: 0
Current number of RX queues: 1
Max possible RX queues: 1
Max possible number of RXDs per queue: 32768
Min possible number of RXDs per queue: 32
RXDs number alignment: 1
Current number of TX queues: 1
Max possible TX queues: 1
Max possible number of TXDs per queue: 32768
Min possible number of TXDs per queue: 32
TXDs number alignment: 1
Max segment number per packet: 65535
Max segment number per MTU/TSO: 65535
Device capabilities: 0x0( )

********************* Infos for port 1  *********************
MAC address: 52:54:00:AC:4D:41
Device name: 08:00.0
Driver name: net_virtio
Firmware-version: not available
Devargs:
Connect to socket: 0
memory allocation on the socket: 0
Link status: up
Link speed: Unknown
Link duplex: full-duplex
Autoneg status: On
MTU: 1500
Promiscuous mode: disabled
Allmulticast mode: enabled
Maximum number of MAC addresses: 64
Maximum number of MAC addresses of hash filtering: 0
VLAN offload:
  strip off, filter off, extend off, qinq strip off
No RSS offload flow type is supported.
Minimum size of RX buffer: 64
Maximum configurable length of RX packet: 9728
Maximum configurable size of LRO aggregated packet: 0
Current number of RX queues: 1
Max possible RX queues: 1
Max possible number of RXDs per queue: 32768
Min possible number of RXDs per queue: 32
RXDs number alignment: 1
Current number of TX queues: 1
Max possible TX queues: 1
Max possible number of TXDs per queue: 32768
Min possible number of TXDs per queue: 32
TXDs number alignment: 1
Max segment number per packet: 65535
Max segment number per MTU/TSO: 65535
Device capabilities: 0x0( )
testpmd>
testpmd> show config fwd
mac packet forwarding - ports=2 - cores=1 - streams=2 - NUMA support enabled, MP allocation mode: native
Logical Core 1 (socket 0) forwards packets on 2 streams:
  RX P=0/Q=0 (socket 0) -> TX P=1/Q=0 (socket 0) peer=12:34:56:78:9A:BC
  RX P=1/Q=0 (socket 0) -> TX P=0/Q=0 (socket 0) peer=12:34:56:78:9A:BC

testpmd> start
mac packet forwarding - ports=2 - cores=1 - streams=2 - NUMA support enabled, MP allocation mode: native
Logical Core 1 (socket 0) forwards packets on 2 streams:
  RX P=0/Q=0 (socket 0) -> TX P=1/Q=0 (socket 0) peer=12:34:56:78:9A:BC
  RX P=1/Q=0 (socket 0) -> TX P=0/Q=0 (socket 0) peer=12:34:56:78:9A:BC

  mac packet forwarding packets/burst=32
  nb forwarding cores=1 - nb forwarding ports=2
  port 0: RX queue number: 1 Tx queue number: 1
    Rx offloads=0x0 Tx offloads=0x0
    RX queue: 0
      RX desc=1024 - RX free threshold=0
      RX threshold registers: pthresh=0 hthresh=0  wthresh=0
      RX Offloads=0x0
    TX queue: 0
      TX desc=1024 - TX free threshold=0
      TX threshold registers: pthresh=0 hthresh=0  wthresh=0
      TX offloads=0x0 - TX RS bit threshold=0
  port 1: RX queue number: 1 Tx queue number: 1
    Rx offloads=0x0 Tx offloads=0x0
    RX queue: 0
      RX desc=1024 - RX free threshold=0
      RX threshold registers: pthresh=0 hthresh=0  wthresh=0
      RX Offloads=0x0
    TX queue: 0
      TX desc=1024 - TX free threshold=0
      TX threshold registers: pthresh=0 hthresh=0  wthresh=0
      TX offloads=0x0 - TX RS bit threshold=0
testpmd>
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 6          RX-missed: 0          RX-bytes:  252
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          128
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 6          TX-errors: 0          TX-bytes:  252

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:          128
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 11         RX-missed: 0          RX-bytes:  462
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          296
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 11         TX-errors: 0          TX-bytes:  462

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:          296
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 15         RX-missed: 0          RX-bytes:  630
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 0          TX-errors: 0          TX-bytes:  0

  Throughput (since last show)
  Rx-pps:            1          Rx-bps:          336
  Tx-pps:            0          Tx-bps:            0
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 0          RX-missed: 0          RX-bytes:  0
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 15         TX-errors: 0          TX-bytes:  630

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            1          Tx-bps:          336
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 21         RX-missed: 0          RX-bytes:  882
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 5          TX-errors: 0          TX-bytes:  210

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          184
  Tx-pps:            0          Tx-bps:          152
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 5          RX-missed: 0          RX-bytes:  210
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 21         TX-errors: 0          TX-bytes:  882

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          152
  Tx-pps:            0          Tx-bps:          184
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 21         RX-missed: 0          RX-bytes:  882
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 6          TX-errors: 0          TX-bytes:  252

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:          208
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 6          RX-missed: 0          RX-bytes:  252
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 21         TX-errors: 0          TX-bytes:  882

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          208
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 21         RX-missed: 0          RX-bytes:  882
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 9          TX-errors: 0          TX-bytes:  378

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            1          Tx-bps:          416
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 9          RX-missed: 0          RX-bytes:  378
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 21         TX-errors: 0          TX-bytes:  882

  Throughput (since last show)
  Rx-pps:            1          Rx-bps:          416
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 21         RX-missed: 0          RX-bytes:  882
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 11         TX-errors: 0          TX-bytes:  462

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            0          Tx-bps:          304
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 11         RX-missed: 0          RX-bytes:  462
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 21         TX-errors: 0          TX-bytes:  882

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:          304
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> show port stats all

  ######################## NIC statistics for port 0  ########################
  RX-packets: 21         RX-missed: 0          RX-bytes:  882
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 13         TX-errors: 0          TX-bytes:  546

  Throughput (since last show)
  Rx-pps:            0          Rx-bps:            0
  Tx-pps:            1          Tx-bps:          336
  ############################################################################

  ######################## NIC statistics for port 1  ########################
  RX-packets: 13         RX-missed: 0          RX-bytes:  546
  RX-errors: 0
  RX-nombuf:  0
  TX-packets: 21         TX-errors: 0          TX-bytes:  882

  Throughput (since last show)
  Rx-pps:            1          Rx-bps:          336
  Tx-pps:            0          Tx-bps:            0
  ############################################################################
testpmd> quit
Telling cores to stop...
Waiting for lcores to finish...

  ---------------------- Forward statistics for port 0  ----------------------
  RX-packets: 21             RX-dropped: 0             RX-total: 21
  TX-packets: 17             TX-dropped: 0             TX-total: 17
  ----------------------------------------------------------------------------

  ---------------------- Forward statistics for port 1  ----------------------
  RX-packets: 17             RX-dropped: 0             RX-total: 17
  TX-packets: 21             TX-dropped: 0             TX-total: 21
  ----------------------------------------------------------------------------

  +++++++++++++++ Accumulated forward statistics for all ports+++++++++++++++
  RX-packets: 38             RX-dropped: 0             RX-total: 38
  TX-packets: 38             TX-dropped: 0             TX-total: 38
  ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

Done.

Stopping port 0...
Stopping ports...
Done

Stopping port 1...
Stopping ports...
Done

Shutting down port 0...
Closing ports...
Port 0 is closed
Done

Shutting down port 1...
Closing ports...
Port 1 is closed
Done

Bye...
[dpdk@localhost dpdk-stable-21.11.2-backup]$
[dpdk@localhost dpdk-stable-21.11.2-backup]$