Texas Instruments X-Loader 1.41
Starting OS Bootloader...

U-Boot 1.3.3-svn333 (Sep 10 2009 - 16:49:01)

OMAP3530-GP rev 2, CPU-OPP2 L3-165MHz
OMAP3 DevKit8000 Board + LPDDR/NAND
DRAM:  128 MB
NAND:  128 MiB
In:    serial
Out:   serial
Err:   serial
Hit any key to stop autoboot:  0
OMAP3 DevKit8000 # setenv bootargs 'console=ttyS2,115200n8 root=/dev/mmcblk0p3 r
ootdelay=1'
OMAP3 DevKit8000 # mmcinit
OMAP3 DevKit8000 # fatload mmc 0 80300000 uImage
reading uImage

2127220 bytes read
OMAP3 DevKit8000 # bootm 80300000
## Booting kernel from Legacy Image at 80300000 ...
   Image Name:   Linux-2.6.28-rc9-omap1
   Image Type:   ARM Linux Kernel Image (uncompressed)
   Data Size:    2127156 Bytes =  2 MB
   Load Address: 80008000
   Entry Point:  80008000
   Verifying Checksum ... OK
   Loading Kernel Image ... OK
OK

Starting kernel ...

Uncompressing Linux.............................................................
............................................................................ don
e, booting the kernel.
Linux version 2.6.28-rc9-omap1 (luofc@LINUXSERVER) (gcc version 4.2.1 (CodeSourc
ery Sourcery G++ Lite 2007q3-51)) #1 Thu Nov 5 17:42:50 CST 2009
CPU: ARMv7 Processor [411fc083] revision 3 (ARMv7), cr=10c5387f
CPU: VIPT nonaliasing data cache, VIPT nonaliasing instruction cache
Machine: OMAP3 Beagle Board
Memory policy: ECC disabled, Data cache writeback
OMAP3430 Unknown revision

SRAM: Mapped pa 0x40200000 to va 0xd7000000 size: 0x100000
Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 32512
Kernel command line: console=ttyS2,115200n8 root=/dev/mmcblk0p3 rootdelay=1
Clocking rate (Crystal/DPLL/ARM core): 26.0/266/500 MHz
GPMC revision 5.0
IRQ: Found an INTC at 0xd8200000 (revision 4.0) with 96 interrupts
Total of 96 interrupts on 1 active controller
OMAP34xx GPIO hardware version 2.5
PID hash table entries: 512 (order: 9, 2048 bytes)
OMAP clockevent source: GPTIMER12 at 32768 Hz
Console: colour dummy device 80x30
Dentry cache hash table entries: 16384 (order: 4, 65536 bytes)
Inode-cache hash table entries: 8192 (order: 3, 32768 bytes)
Memory: 128MB = 128MB total
Memory: 125340KB available (3908K code, 352K data, 156K init)
Calibrating delay loop... 478.91 BogoMIPS (lpj=1867776)
Mount-cache hash table entries: 512
CPU: Testing write buffer coherency: ok
net_namespace: 288 bytes
NET: Registered protocol family 16
Found NAND on CS0
Registering NAND on CS0
omap3evmdc: Driver registration complete
OMAP DMA hardware revision 4.0
USB: No board-specific platform config found
OMAP DSS rev 2.0
OMAP DISPC rev 3.0
OMAP VENC rev 2
i2c_omap i2c_omap.1: bus 1 rev3.12 at 2600 kHz
twl4030: PIH (irq 7) chaining IRQs 368..375
twl4030: power (irq 373) chaining IRQs 376..383
twl4030: gpio (irq 368) chaining IRQs 384..401
i2c_omap i2c_omap.2: bus 2 rev3.12 at 400 kHz
i2c_omap i2c_omap.3: bus 3 rev3.12 at 400 kHz
SCSI subsystem initialized
twl4030_usb twl4030_usb: Initialized TWL4030 USB module
usbcore: registered new interface driver usbfs
usbcore: registered new interface driver hub
usbcore: registered new device driver usb
musb_hdrc: version 6.0, musb-dma, otg (peripheral+host), debug=0
musb_hdrc: USB OTG mode controller at d80ab000 using DMA, IRQ 92
NET: Registered protocol family 2
IP route cache hash table entries: 1024 (order: 0, 4096 bytes)
TCP established hash table entries: 4096 (order: 3, 32768 bytes)
TCP bind hash table entries: 4096 (order: 2, 16384 bytes)
TCP: Hash tables configured (established 4096 bind 4096)
TCP reno registered
NET: Registered protocol family 1
NetWinder Floating Point Emulator V0.97 (double precision)
VFS: Disk quotas dquot_6.5.1
Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
JFFS2 version 2.2. (NAND) Â© 2001-2006 Red Hat, Inc.
msgmni has been set to 245
alg: No test for stdrng (krng)
io scheduler noop registered
io scheduler anticipatory registered (default)
io scheduler deadline registered
io scheduler cfq registered
Serial: 8250/16550 driver4 ports, IRQ sharing enabled
serial8250.0: ttyS0 at MMIO 0x4806a000 (irq = 72) is a ST16654
serial8250.0: ttyS1 at MMIO 0x4806c000 (irq = 73) is a ST16654
serial8250.0: ttyS2 at MMIO 0x49020000 (irq = 74) is a ST16654
console [ttyS2] enabled
brd: module loaded
loop: module loaded
dm9000 Ethernet Driver, V1.31
eth0: dm9000a at c88ae000,c88b2400 IRQ 185 MAC: 00:11:22:33:44:55 (chip)
Linux video capture interface: v2.00
tvp514x 2-005d: Registered to v4l2 master omap34xxcam!!
i2c /dev entries driver
Driver 'sd' needs updating - please use bus_type methods
omap2-nand driver initializing
NAND device: Manufacturer ID: 0x2c, Chip ID: 0xb1 (Micron NAND 128MiB 1,8V 16-bi
t)
cmdlinepart partition parsing not available
Creating 5 MTD partitions on "omap2-nand":
0x00000000-0x00080000 : "X-Loader"
0x00080000-0x00260000 : "U-Boot"
0x00260000-0x00280000 : "U-Boot Env"
0x00280000-0x00680000 : "Kernel"
0x00680000-0x08000000 : "File System"
usbmon: debugfs is not available
ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver
ehci-omap ehci-omap.0: OMAP-EHCI Host Controller
ehci-omap ehci-omap.0: new USB bus registered, assigned bus number 1
ehci-omap ehci-omap.0: irq 77, io mem 0x48064800
ehci-omap ehci-omap.0: USB 2.0 started, EHCI 1.00
usb usb1: configuration #1 chosen from 1 choice
hub 1-0:1.0: USB hub found
hub 1-0:1.0: 3 ports detected
Initializing USB Mass Storage driver...
usbcore: registered new interface driver usb-storage
USB Mass Storage support registered.
g_ether gadget: using random self ethernet address
g_ether gadget: using random host ethernet address
usb0: MAC 8a:b8:89:86:8c:20
usb0: HOST MAC a2:bc:af:f4:ca:bd
g_ether gadget: Ethernet Gadget, version: Memorial Day 2008
g_ether gadget: g_ether ready
musb_hdrc musb_hdrc: MUSB HDRC host driver
musb_hdrc musb_hdrc: new USB bus registered, assigned bus number 2
usb usb2: configuration #1 chosen from 1 choice
hub 2-0:1.0: USB hub found
hub 2-0:1.0: 1 port detected
input: omap_twl4030keypad as /class/input/input0
input: gpio-keys as /class/input/input1
ads7846 spi2.0: touchscreen, irq 187
input: ADS784x Touchscreen as /class/input/input2
twl4030_rtc twl4030_rtc: rtc core: registered twl4030_rtc as rtc0
twl4030_rtc twl4030_rtc: Power up reset detected.
twl4030_rtc twl4030_rtc: Enabling TWL4030-RTC.
Registered led device: led1
Registered led device: led2
Registered led device: ledB
Registered led device: led3
usbcore: registered new interface driver usbhid
usbhid: v2.6:USB HID core driver
Advanced Linux Sound Architecture Driver Version 1.0.18rc3.
ASoC version 0.13.2
OMAP3 omap3devkit9100 SoC init
TWL4030 Audio Codec init
asoc: twl4030 <-> omap-mcbsp-dai-(link_id) mapping ok
ALSA device list:
  #0: omap3devkit9000 (twl4030)
TCP cubic registered
NET: Registered protocol family 17
NET: Registered protocol family 15
RPC: Registered udp transport module.
RPC: Registered tcp transport module.
Power Management for TI OMAP3.
VFP support v0.3: implementor 41 architecture 3 part 30 variant c rev 1
omapfb: using mode 4.3inch_LCD
Console: switching to colour frame buffer device 60x34
clock: clksel_round_rate_div: dpll4_m4_ck target_rate 28800000
clock: new_div = 15, new_rate = 28800000
tvp514x 2-005d: Write: retry ... 0
tvp514x 2-005d: Write: retry ... 1
tvp514x 2-005d: Write: retry ... 2
tvp514x 2-005d: Write: retry ... 3
tvp514x 2-005d: Write: retry ... 4
tvp514x 2-005d: Write: retry ... 5
mmc0: new high speed SDHC card at address 871d
tvp514x 2-005d: Write: retry ... 0
mmcblk0: mmc0:871d SD08G 3.42 GiB
 mmcblk0: p1 p2 p3
tvp514x 2-005d: Write: retry ... 1
tvp514x 2-005d: Write: retry ... 2
tvp514x 2-005d: Write: retry ... 3
tvp514x 2-005d: Write: retry ... 4
tvp514x 2-005d: Write: retry ... 5
tvp514x 2-005d: chip id mismatch msb:0x87 lsb:0x87
tvp514x 2-005d: Unable to detect decoder
tvp514x 2-005d: Write: retry ... 0
tvp514x 2-005d: Write: retry ... 1
tvp514x 2-005d: Write: retry ... 2
tvp514x 2-005d: Write: retry ... 3
tvp514x 2-005d: Write: retry ... 4
tvp514x 2-005d: Write: retry ... 5
tvp514x 2-005d: Write: retry ... 0
tvp514x 2-005d: Write: retry ... 1
tvp514x 2-005d: Write: retry ... 2
tvp514x 2-005d: Write: retry ... 3
tvp514x 2-005d: Write: retry ... 4
tvp514x 2-005d: Write: retry ... 5
tvp514x 2-005d: chip id mismatch msb:0x87 lsb:0x87
tvp514x 2-005d: Unable to detect decoder
tvp514x 2-005d: Write: retry ... 0
tvp514x 2-005d: Write: retry ... 1
tvp514x 2-005d: Write: retry ... 2
tvp514x 2-005d: Write: retry ... 3
tvp514x 2-005d: Write: retry ... 4
tvp514x 2-005d: Write: retry ... 5
tvp514x 2-005d: Write: retry ... 0
tvp514x 2-005d: Write: retry ... 1
tvp514x 2-005d: Write: retry ... 2
tvp514x 2-005d: Write: retry ... 3
tvp514x 2-005d: Write: retry ... 4
tvp514x 2-005d: Write: retry ... 5
tvp514x 2-005d: chip id mismatch msb:0x87 lsb:0x87
tvp514x 2-005d: Unable to detect decoder
tvp514x 2-005d: Write: retry ... 0
tvp514x 2-005d: Write: retry ... 1
tvp514x 2-005d: Write: retry ... 2
tvp514x 2-005d: Write: retry ... 3
tvp514x 2-005d: Write: retry ... 4
tvp514x 2-005d: Write: retry ... 5
tvp514x 2-005d: Write: retry ... 0
tvp514x 2-005d: Write: retry ... 1
tvp514x 2-005d: Write: retry ... 2
tvp514x 2-005d: Write: retry ... 3
tvp514x 2-005d: Write: retry ... 4
tvp514x 2-005d: Write: retry ... 5
tvp514x 2-005d: chip id mismatch msb:0x87 lsb:0x87
tvp514x 2-005d: Unable to detect decoder
Display already enabled
Buffer Size = 3686400
omap_vout: registered and initialized                   video device 0 [v4l2]
Buffer Size = 3686400
omap_vout: registered and initialized                   video device 1 [v4l2]
display->updated
twl4030_rtc twl4030_rtc: setting system clock to 2000-01-01 00:00:01 UTC (946684
801)
Waiting 1sec before mounting root device...
kjournald starting.  Commit interval 5 seconds
EXT3 FS on mmcblk0p3, internal journal
EXT3-fs: mounted filesystem with ordered data mode.
VFS: Mounted root (ext3 filesystem).
Freeing init memory: 156K
                Welcome to Meego
[  OK  ]
udevd-work[521]: error opening ATTR{/sys/class/sound/controlC0/../uevent} for wr
iting: No such file or directory

mount: mount point /sys/kernel/debug/ does not exist

MeeGo release 1.0.80 (MeeGo)
Kernel 2.6.28-rc9-omap1 on an armv7l

localhost.localdomain login: vijay
Password:
Last login: Sat Jan  1 00:02:54 on ttyS2
[vijay@localhost ~]$
[vijay@localhost ~]$
[vijay@localhost ~]$
[vijay@localhost ~]$
[vijay@localhost ~]$ twm-session
/usr/bin/xsetroot:  unable to open display ''
/usr/bin/twm:  unable to open display ""
/usr/bin/xterm Xt error: Can't open display:
/usr/bin/xterm:  DISPLAY is not set
[vijay@localhost ~]$ export DISPALY=:0
[vijay@localhost ~]$ twm-session
/usr/bin/xsetroot:  unable to open display ''
/usr/bin/twm:  unable to open display ""
/usr/bin/xterm Xt error: Can't open display:
/usr/bin/xterm:  DISPLAY is not set
[vijay@localhost ~]$